;*********************************************************************************************
; Windows USB Android Debug Bridge (ADB) Setup File for Intel Android Smartphones
;
; Copyright (c) 2012 Intel Corporation 
;
; For use only on Windows operating systems.
;
; (modified by stv.  2013-07-10)
;
;*********************************************************************************************

[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer			= 04/30/2012,1.2.0.0
CatalogFile.NTx86  	= intc_adbx86.cat
CatalogFile.NTAMD64 = intc_adbamd64.cat

;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%ProviderName% = Generic, NTx86.6.0, NTamd64.6.0

[Generic]
; Intel Clovertrail Android ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_0A14
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A16&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A18&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1A&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1B&MI_04
; Intel Medfield Android ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09EF
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FC&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FE&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F8&MI_04
; Intel Medfield Android GingerBread
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F1
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F6
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F1&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F2&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_8087&PID_0FFF

[Generic.NTx86.6.0]
; Intel Clovertrail Android ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_0A14
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A16&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A18&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1A&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1B&MI_04
; Intel Medfield Android ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09EF
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FC&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FE&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F8&MI_04


; Intel Medfield Android GingerBread
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F1
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F6
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F1&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F2&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A25&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_8087&PID_0FFF

[Generic.NTamd64.6.0]
; Intel Clovertrail Android ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_0A14
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A16&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A18&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1A&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A1B&MI_04
; Intel Medfield ICS
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09EF
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FC&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09FE&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F8&MI_04
; Intel Medfield GingerBread
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F1
%SingleAdbInterface% = USB_Install, USB\VID_8087&PID_09F6
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F1&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F2&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F4&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_09F6&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_8087&PID_0A25&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_8087&PID_0FFF

[USB_Install]
Include = winusb.inf
Needs = WINUSB.NT

[USB_Install.Services]
Include = winusb.inf
AddService = WinUSB, 0x00000002, WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName = %WinUSB_SvcDesc%
ServiceType = 1
StartType = 3
ErrorControl = 1
ServiceBinary = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion = 1.9

[USB_Install.HW]
AddReg = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles = 11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName              = "Intel Corporation"
SingleAdbInterface        = "Intel Android ADB Interface"
CompositeAdbInterface     = "Intel Android Composite ADB Interface"
SingleBootLoaderInterface = "Intel Android Bootloader Interface"
WinUSB_SvcDesc            = "Intel Android USB Driver"
DISK_NAME                 = "Intel Android WinUsb installation disk"
ClassName                 = "Intel Android Phone"

