;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 12/02/2013,8.0.0000.1
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat

[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1


[Manufacturer]
%ProviderName% = ASUS, NTx86, NTamd64

[ASUS.NTx86]
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C81&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C83&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C85&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C91&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C93&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C95&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D05&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_4DAE
%SingleBootLoaderInterface% = USB_Install, USB\VID_0B05&PID_4DAF
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4DDE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4DEF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E05&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E1F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E3F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E5F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F3F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F5F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F7F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4FBF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_503F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_505F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_507F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_50BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_513F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_515F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_517F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_519F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5201&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5203&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5205&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5207&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5211&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5213&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5215&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_521F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5221&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5223&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5225&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5231&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5233&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5235&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_523F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5241&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5243&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5245&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5251&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5253&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5255&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_525F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5261&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5263&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5265&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5271&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5273&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5275&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_531F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_533F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_535F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5401
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5411&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5413&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5416&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5418&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_541F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_543F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_545F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5461
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5466&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5467&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5468&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5469&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5471
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5477&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5479&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5481&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5483&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5485&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5491&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5493&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5495&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5501&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5503&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_551F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_553F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_555F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_561F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_563F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_565F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_571F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_573F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_575F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_581F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_583F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_585F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_591F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_593F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_595F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_7770
%SingleBootLoaderInterface% = USB_Install, USB\VID_0B05&PID_7771
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7773&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7775&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7777&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7781&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7783&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7785&MI_01

[ASUS.NTamd64]
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C81&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C83&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C85&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C91&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C93&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4C95&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CA5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CB5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CC5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CD5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4CE5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4D05&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_4DAE
%SingleBootLoaderInterface% = USB_Install, USB\VID_0B05&PID_4DAF
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4DDE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4DEF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E05&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E1F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E3F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4E5F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F3F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F5F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4F7F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_4FBF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_503F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_505F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_507F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_50BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_513F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_515F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_517F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_519F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5201&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5203&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5205&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5207&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5211&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5213&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5215&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_521F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5221&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5223&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5225&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5231&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5233&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5235&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_523F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5241&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5243&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5245&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5251&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5253&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5255&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_525F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5261&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5263&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5265&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5271&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5273&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5275&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_531F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_533F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_535F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5401
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5411&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5413&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5416&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5418&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_541F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_543F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_545F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5461
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5466&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5467&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5468&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5469&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_5471
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5477&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5479&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5481&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5483&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5485&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5491&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5493&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5495&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5501&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_5503&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_551F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_553F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_555F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_561F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_563F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_565F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_571F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_573F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_575F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_581F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_583F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_585F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_591F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_593F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_595F&MI_01
%SingleAdbInterface% = USB_Install, USB\VID_0B05&PID_7770
%SingleBootLoaderInterface% = USB_Install, USB\VID_0B05&PID_7771
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7773&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7775&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7777&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7781&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7783&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0B05&PID_7785&MI_01

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "ASUSTeK COMPUTER INC."
SingleAdbInterface          = "ASUS Android ADB Interface"
CompositeAdbInterface       = "ASUS Android Composite ADB Interface"
SingleBootLoaderInterface   = "ASUS Android Bootloader Interface"
WinUSB_SvcDesc              = "ASUS Android USB Driver"
DISK_NAME                   = "ASUS Android WinUsb installation disk"
ClassName                   = "ASUS Android Device"
